**M S Ramaiah Institute of Technology**

(An Autonomous Institute, Affiliated to VTU)

MSR Nagar, MSRIT post, Bangalore-54.

An **Implementation Document** for

**BUILDING A WEB SERVICE FRAMEWORK (STOW-RS) FOR MEDICAL IMAGING (DICOM)**

**Submitted By:**

**NEHA PATHAPATI**

**(USN:** 1MS12CS143)

**COMPANY:** PHILIPS

**BUSINESS UNIT:** HEALTH SYSTEMS

*in partial fulfillment for the award of the degree of*

# *Bachelor of Engineering in Computer Science & Engineering*



**DEPARTMENT OF COMPUTER SCIENCE & ENGINEERING**

**M.S.RAMAIAH INSTITUTE OF TECHNOLOGY**

**(Autonomous Institute, Affiliated to VTU)**

**BANGALORE-560054**

[www.msrit.edu](http://www.msrit.edu), **Feb 2016**

**IMPLEMENTATION**

**I.TOOLS INTRODUCTION**

Our project involves the building of STOW-RS. STOW-RS is a restful service that facilitates third party clients to store DICOM (Digital Imaging and Communication in Medicine) files over the PACS (Picture Archival and Communication System).

Several tools were employed during the requirement gathering, planning, design, implementation, and testing phases of STOW-RS. A brief description of these tools is given below:

1. **GANNT PROJECT**

In project management, a schedule is a listing of a project's milestones, activities, and deliverables, usually with intended start and finish dates. Project scheduling is a critical activity in the execution of any software project. Scheduling of tasks of STOW-RS was depicted using Gantt Charts. These Gantt Charts were generated with the help of the Gantt Project tool. Gantt Project is GPL-licensed, Java based, project management software that runs under the Windows, Linux and Mac OS X operating systems. The generated schedule was then exported into a pdf and circulated to the team member’s.

1. **StarUML**

Software design is a process to transform user requirements into some suitable form, which helps the programmer in software coding and implementation. The output of the design process can directly be streamlined into implementation in programming languages. Software design is the first step in Software Design Life Cycle, which moves the concentration from problem domain to solution domain. A precise understanding of the implementation of the STOW restful service was obtained by creating the Architectural View, Component View, Logical View (Sequence Diagram and the Class Diagram), and the Deployment View of STOW-RS. StarUML was the tool employed to create these software design diagrams.

The Unified Modeling Language (UML) is a widely used design notation for software. StarUML is a software modeling platform that supports UML. It is based on UML version 1.4 and provides eleven different types of diagram, and it accepts UML 2.0 notation. It actively supports the MDA (Model Driven Architecture) approach by supporting the UML profile concept. StarUML excels in customizability to the user’s environment and has a high extensibility in its functionality. The diagrams drawn using StarUML could be conveniently exported into a PDF.

1. **VISUAL STUDIO ULTIMATE**

Microsoft Visual Studio is an integrated development environment (IDE) from Microsoft, which apart from enabling users to develop computer programs for Microsoft Windows, also allows creation of UML diagrams.

The Data Flow Diagram of STOW-RS was constructed using Visual Studio 2013.

1. **VISUAL STUDIO 2013**

Microsoft Visual Studio is an integrated development environment (IDE) from Microsoft. It is used to develop computer programs for Microsoft Windows, as well as web sites, web applications and web services. Visual Studio uses Microsoft software development platforms such as Windows API, Windows Forms, Windows Presentation Foundation, Windows Store and Microsoft Silverlight. It can produce both native code and managed code.

Visual Studio includes a code editor supporting IntelliSense (the code completion component) as well as code refactoring. The integrated debugger works both as a source-level debugger and a machine-level debugger. Other built-in tools include a forms designer for building GUI applications, web designer, class designer, and database schema designer. It accepts plug-ins that enhance the functionality at almost every level—including adding support for source-control systems and adding new toolsets like editors and visual designers for domain-specific languages or toolsets for other aspects of the software development lifecycle (like the Team Foundation Server client: Team Explorer).

Visual Studio supports different programming languages and allows the code editor and debugger to support (to varying degrees) nearly any programming language, provided a language-specific service exists. Built-in languages include C, C++, C++/CLI (via Visual C++), VB.NET (via Visual Basic .NET), C# (via Visual C#), and F#. Support for other languages such as Python, Ruby, Node.js, and M among others is available via language services installed separately. It also supports XML/XSLT, HTML/XHTML, JavaScript and CSS. Java (and J#) were supported in the past**.**

The security layer, the Rest API, and the DICOM layer of STOW-RS were coded in C# 4.5. The Storage Library was written in C++/CLI. Visual Studio 2013 was employed for all development tasks of STOW-RS.

1. **FIDDLER**

Fiddler is an HTTP debugging proxy server application. Fiddler captures HTTP and HTTPS traffic and logs it for the user to review. Any browser or web application (and most mobile devices) can be configured to route its traffic through Fiddler.

As STOW-RS forms the server side of the web service, there is no typical GUI developed. However, during development of STOW-RS, the client accessing the STOW-RS service is simulated/mocked using the Fiddler Tool. The client’s request to store a DICOM file on the STOW server is triggered using the Fiddler Tool. The HTTP response returned by the server to the client is also viewed using Fiddler.

1. **MicroDicom VIEWER**

MicroDicom is application for primary processing and preservation of medical images in DICOM format. It is equipped with most common tools for manipulation of DICOM images and it has an intuitive user interface. Also, it has the advantage of being open source. Specifically, it allows - opening and saving of medical images in DICOM format, displaying of both the metadata (the header in the form of DICOM tags) and the pixel/bulk data of DICOM files from different studies/ examinations, and loading of DICOM images via drag and drop or double-click in DICOM viewer.

During the development of STOW-RS, this tool was used to read the values of tags in the header of DICOM file and verify the image being stored using this service.

1. **HP FORTIFY SOURCE CODE ANALYZER**

Fortify Source Code Analyzer (SCA) is a set of software security analyzers that search for violations of security‐specific coding rules and guidelines in a variety of languages. The rich data provided by Fortify SCA language technology enables the analyzers to pinpoint and prioritize violations so that fixes can be fast and accurate. The analysis information produced by SCA helps you deliver more secure software, as well as making security code reviews more efficient, consistent, and complete. This is especially advantageous when large code bases are involved. The modular architecture of SCA allows to quickly upload new, third party, and customer‐specific security rules.

At the highest level, using Fortify SCA involves:

* Choosing to run SCA as a stand‐alone process or integrating Fortify SCA as part of the build tool
* Translating the source code into an intermediate translated format, preparing the code base for scanning by the different analyzers
* Scanning the translated code, producing security vulnerability reports
* Auditing the results of the scan, either by transferring the resulting FPR file to Audit Workbench or Fortify 360 Server for analysis, or directly with the results displayed onscreen.

The Fortify SCA plug-in was installed in Visual Studio 2013. Then, the code of STOW-RS was analyzed using the Fortify SCA against the latest set of coding rules defined by Philips. Fortify groups the errors in the code into 4 severity categories - Critical, High, Medium, and Low. A PDF report of the Fortify findings can also be generated.

1. **APACHE JMeter**

Apache JMeter is a 100% pure Java application designed to load test client/server software, such as a web service. It may be used to test performance both on static and dynamic resources such as static files, Java Servlets, ASP.NET, PHP, CGI scripts, Java objects, databases, FTP servers, and more. JMeter can be used to simulate a heavy load on a server, network or object to test its strength or to analyze overall performance under different load types.

The performance of STOW-RS is tested using JMeter - the time taken by STOW-RS to process a client’s request, the responsiveness, speed, scalability, and stability characteristics of STOW-RS for varying DICOM file sizes and concurrent requests that can be processed by STOW-RS.

1. **C++ MEMORY VALIDATOR**

C++ Memory Validator is a memory leak and memory error detection software tool for use by software developers, software quality assurance testers and customer support staff.

Memory Validator is employed to:

* Detect memory leaks and handle leaks.
* Find native memory leaks in mixed-mode .Net applications.
* Find double deletes, double frees and related memory errors.
* Find uninitialized memory in C++ objects.
* Run regression tests to find memory leaks in your overnight builds.
* Monitor billions of allocations in your application.
* Memory leaks in the C++/CLI code of Storage Library were detected using the Memory Validator tool.

**10). HP FORTIFY MEMORY PROFILER**

The static memory leaks in C# code are detected using the HP Fortify Memory Profiler.

**11). TEAM FOUNDATION SERVER (TFS)**

Team Foundation Server provides a set of collaboration tools that work with your existing IDE or editor, so your team can work effectively on software projects of all shapes and sizes. It is a Microsoft product that provides source code management, reporting, and requirements management, project management for agile software development, automated builds, and lab management, testing and release management capabilities. It covers the entire application lifecycle. TFS can be used as a back-end to numerous integrated development environments (IDEs) but is tailored for Microsoft Visual Studio and Eclipse on all platforms.

Some of the functions of TFS include:

* Version control

Unlimited, private, and secure version control is ensured using TFS. Storage and collaboration on code with unlimited private repositories is possible. Team Foundation version control (TFVC) enables centralized version control. Collaboration on code occurs easily with pull requests and code reviews, while defining and managing permissions to secure your repositories.

* Continuous integration

TFS facilitates catching quality issues early with continuous integration (CI) builds that compile and test applications automatically after any code change.

* Integration

TFS makes it easy to integrate your custom tool or third-party service with Team Foundation Server using open standards like REST APIs and OAuth 2.0. A set of ready-made integrations that can be easily configured from the account dashboard are also supported.

* Tools for Agile Teams

TFS allows to capture, prioritize, and track work with backlogs and customizable Kanban boards. Work items link directly to code to ensure transparency, and can be used to build rich dashboards for easy reporting.

For each feature to be developed, user stories are added to the TFS. Tasks are then added to these user stories. Each member of the team is assigned work in terms of tasks under one or more user stories. The team member is allowed to change the status of his tasks to “Completed” when done.

* Backlogs

They allow to quickly define, prioritize, and decompose the work in the project. Prioritization is easy with drag-and-drop re-ordering helping to keep the most important work at the top of your backlog.

* Scrum

Planning of sprints using team-based capacity planning, assign work by dragging-dropping, and monitor progress throughout the sprint with real-time burndown charts can be done.

* Kanban board

Each backlog in Visual Studio Team Services comes with a built-in Kanban board. Customizing the columns to suit workflows, setting WIP limits to monitor flow, and drag-and-drop items through the correct columns as work starts and finishes can be done.

* Dashboards

Dashboards provide visibility to the team and the stakeholders. Visual Studio Team Services is used to get everyone on the same page.

* Taskboards

Helps to organize efficient stand-up meetings. A sprint is run using a fit-for-purpose Taskboard where the work can be watched as it happens. Pivoting the board by team member or story enables daily standups to be quick and efficient.

* Connected to Code

All code changes are linked directly to the story, bug, or task driving the work. Visual Studio Team Services provides unparalleled traceability and visibility to the evolving codebase.

* Charts

Build charts that bring your data to life and make it visible to your team, organization, and stakeholders. Start from a query and then build a chart that highlights work needing attention.

* Forecast

Look ahead using simple forecasting on your backlog. Agile is about being ready for change. Visual Studio Team Services gives you the visibility and awareness to make the right decision at the right time.

* Tracking

Queries let you track and organize data to fit the needs of every project and every situation. Creation custom queries to look for stale work, impediments blocking progress, or backlog items that need attention can be done.

* Code check-in

A developer’s code can be checked in to the TFS for other developers in the team to review and integrate.

**12). NUNIT TESTING**

NUnit is an open source unit testing framework for Microsoft .NET. It serves the same purpose as JUnit does in the Java world, and is one of many programs in the xUnit family. NUnit is a commonly used framework for all .Net languages. Initially ported from JUnit, the current production release, version 3.0, has been completely rewritten with many new features and support for a wide range of .NET platforms. Some of the features of NUnit framework include:

* Tests can be run from a console runner, within Visual Studio through a Test Adapter or through 3rd party runners.
* Tests can be run in parallel.
* Strong support for data driven tests.
* Supports multiple platforms including .NET Core.
* Every test case can be added to one or more categories, to allow for selective running.

The individual functions of Storage Library were tested using NUnit testing framework by the developers.

**13). NCover**

NCover is a .NET code coverage tool. There are two non-related NCover products that do .NET code coverage. There is an open source NCover that can be found on Sourceforge and there is a company called NCover, LLC.

**14). STENTOR LOGGING**

Stentor Logging is a set of libraries that enable logging of several types of messages – Critical, Error, Debug, Warning, and Informational.

**II. TECHNOLOGY INTRODUCTION**

The technologies we were introduced to during the development of STOW-RS include the following:

1. **C# AND .NET FRAMEWORK 4.5**

C# (pronounced as see sharp) is a multi-paradigm programming language encompassing strong typing, imperative, declarative, functional, generic, object-oriented, and component-oriented programming disciplines. It was developed by Microsoft within its .NET initiative. C# is one of the programming languages designed for the Common Language Infrastructure. In simple terms, C# is a general-purpose, object-oriented programming language. C# programs run on the .NET Framework, an integral component of Windows that includes a virtual execution system called the common language runtime (CLR) and a unified set of class libraries. The CLR is the commercial implementation by Microsoft of the common language infrastructure (CLI), an international standard that is the basis for creating execution and development environments in which languages and libraries work together seamlessly. The use of managed and unmanaged code in C# was extensively learnt about and exercised.

1. **C++/CLI (C++ MODIFIED FOR COMMON LANGUAGE INFRASTRUCTURE)**

It is a language specification created by Microsoft and intended to supersede Managed Extensions for C++. It is a complete revision that aims to simplify the older Managed C++ syntax. Specifically, the concept of auto-pointers in C++/CLI was rigorously learnt and used.

1. **REST ARCHITECTURE**

REST is a design pattern for implementing networked systems, not a standard. Representational State Transfer (REST) is an architectural style that specifies constraints, such as the uniform interface, that if applied to a web service induce desirable properties, such as performance, scalability, and modifiability that enable services to work best on the Web. In the REST architectural style, data and functionality are considered resources and are accessed using Uniform Resource Identifiers (URIs), typically links on the Web. The resources are acted upon by using a set of simple, well-defined operations. The REST architectural style constrains an architecture to a client/server architecture and is designed to use a stateless communication protocol, typically HTTP. In the REST architecture style, clients and servers exchange representations of resources by using a standardized interface and protocol.

1. **TRANSPORT LAYER SECURITY USING SSL CERTIFICATES**

Transport Layer Security (TLS) and its predecessor, Secure Sockets Layer (SSL), both of which are frequently referred to as 'SSL', are cryptographic protocols that provide communications security over a computer network. The primary goal of the TLS protocol is to provide privacy and data integrity between two communicating computer applications. When secured by TLS, connections between a client) and a server have one or more of the following properties:

* The connection is private because symmetric cryptography is used to encrypt the data transmitted. The keys for this symmetric encryption are generated uniquely for each connection and are based on a shared secret negotiated at the start of the session. The server and client negotiate the details of which encryption algorithm and cryptographic keys to use before the first byte of data is transmitted (see Algorithm). The negotiation of a shared secret is both secure (the negotiated secret is unavailable to eavesdroppers and cannot be obtained, even by an attacker who places himself in the middle of the connection) and reliable (no attacker can modify the communications during the negotiation without being detected).
* The identity of the communicating parties can be authenticated using public-key cryptography.
* The connection is reliable because each message transmitted includes a message integrity check using a message authentication code to prevent undetected loss or alteration of the data during transmission.

TLS can be ensured by ensuring that all communication between client and server occurs through the use of HTTPS protocol. To achieve this, a HTTPS URL is registered at the server site for the client to access. Then, the client and server SSL certificates are configured appropriately at the respective client and server locations. Then, the thumbprint of the server certificate is bound to a port and the GUID of a Visual Studio application. The authorized client can now access the service through a secure URL.

1. **UNIT TESTING**

Unit testing is a software development process in which the smallest testable parts of an application, called units, are individually and independently scrutinized for proper operation. The primary goal of unit testing is to take the smallest piece of testable software in the application, isolate it from the remainder of the code, and determine whether it behaves exactly as you expect. Each unit is tested separately before integrating them into modules to test the interfaces between modules. Unit testing using NUnit Framework was done. Unit testing facilitates test driven development.

1. **DICOM (DIGITAL IMAGING AND COMMUNICATIN IN MEDICINE)**

DICOM is a standard for handling, storing, printing, and transmitting information in medical imaging. It includes a file format definition and a network communications protocol. The communication protocol is an application protocol that uses TCP/IP to communicate between systems. DICOM files can be exchanged between two entities that are capable of receiving image and patient data in DICOM format. The National Electrical Manufacturers Association (NEMA) holds the copyright to this standard. DICOM enables the integration of scanners, servers, workstations, printers, and network hardware from multiple manufacturers into a picture archiving and communication system (PACS).

**III. OVERALL VIEW OF THE PROJECT IN TERMS OF IMPLEMENTATION**


A block diagram of the STOW - RS service is shown in Figure.1:

**NOTE:** During implementation, the security, REST, and DICOM layer are referred to as STOW-RS. The Storage Library is referred to as the Storage Library. The STOW-RS and the Storage Library were implemented individually and then integrated.

The layers of STOW-RS written in C# include – the security layer, the REST layer, and the DICOM layer.

However, the Storage Library is coded in C++/CLI. The requests to STOW-RS service from the clients and the response from STOW-RS to the clients are managed by HTTP message parsing.

STOW-RS is developed as an add-on for the PACS. STOW-RS is developed independently and then integrated with. These are Web services which expose DICOM standard based REST APIs to save and retrieve DICOM files.



**Figure 1:** ARCHITECTURE OF STOW – RS

A brief overview of the implementation of STOW-RS is as follows:

* The third – party client is the entity external to the healthcare organization that wishes to store DICOM files from the PACS.
* The Security Layer is ensures Transport Layer Security by:
* Mechanism for storing DICOM persistent objects via STOW-RS will be through HTTPS protocol, using DICOM UIDs for Study/Series/SOP Instance level.
* HTTP BASIC Authorization over SSL is supported.
* Deployment of trusted SSL Client and Server Certificates on the client and the sever machine (upon which STOW-RS is deployed). Trusted Client and Server certificates are used for integration and testing purposes only.
* The REST API Interface and Implementation forms the web access layer for the STOW-RS service for storing Dicom files. The REST Interface is the REST API used to enable the client to access STOW – RS service.
* The functionality of the DICOM Library includes:
* Validation of the request and the DICOM files being pushed into PACS by the client.
* Contains implementation of the logging mechanism for better debugging during development of STOW-RS.
* The DICOM Library also encompasses the critical logic concerned with the complexity of transforming the DICOM files present in the body of HTTP Request messages into a suitable form that can be stored on the PACS.
* Issuing of the appropriate HTTP response message based on the status of one or more DICOM files the STOW-RS service has attempted to store on the PACS.
* The Storage Library is responsible for the physical storing of DICOM files, independent of the underlying storage architecture (NAS, SAN, or NFS).

**IV. EXPLANATION OF ALGORITHM AND HOW IT HAS BEEN IMPLEMENTED**

This information is proprietary to Philips. Hence, it cannot be disclosed.

**V. INFORMATION ABOUT IMPLEMENTATION OF MODULES**

At a high level, the modules of STOW-RS and their implementation details are as follows:

**1). Accept STOW requests from third party clients**

* The client requests are received through the REST API.
* All request messages to the STOW-RS server are HTTP/1.1 multipart messages.
* When a single request to the STOW-S service sends more than one DICOM image, each DICOM image is present in one part of the HTTP multipart message.
* The Content-Type field of the HTTP Request Message in an HTTP/1.1 transaction is used by STOW-RS to determine the type of data it is receiving.
* The data types supported by STOW-RS include - application/dicom, application/dicom+xml, and application/json.
* The request message body can contain a DICOM object, metadata and/or bulk data depending on the "Content-Type".
* For development purposes, the Fiddler tool is used to stimulate STOW-RS requests from the client.
* The logic for extracting and processing of the DICOM file present in a HTTP Request Message is written in C#.

The STOW - RS service is developed to process storage requests with the following HTTP header format:

* Resource

{SERVICE}/studies [/{StudyInstanceUID}]

Where,

{SERVICE} is the base URL for the service. This may be a combination of scheme (either HTTP or HTTPS), host, port, and application;

{StudyInstanceUID} (Optional) is the study instance UID for a single study. If not specified, instances can be from multiple studies. If specified, all instances shall be from that study, and instances not matching the StudyInstanceUID shall be rejected.

* Method

POST

* Headers

Content-Type - The representation scheme being posted to the RESTful service. The types allowed for this request header are as follows:

* Multipart/related; type=application/dicom; boundary = {MessageBoundary}
* Multipart/related; type=application/dicom+xml; boundary = {MessageBoundary}.
* The DICOM Request Message has a multipart body.
* Content-Type:

Multipart/related; type=application/dicom; boundary = {MessageBoundary}.

Specifies that the post is XML metadata and bulk data.

* The multipart request body contains every instance to be stored. Each instance is in a separate part of the multipart body.
* Each part in the multipart body represents a DICOM SOP Instance with the following HTTP headers:
* Content-Type: application/dicom.
* The XML Metadata and Bulk Data Request Message has a multipart body.
* Content-Type:

Multipart/related; type=application/dicom+xml; boundary = {MessageBoundary}

* The multipart request body contains all the metadata and bulk data to be stored.
* If the number of bulk data parts does not correspond to the number of unique BulkDataURIs in the metadata then the entire message is invalid and will generate an error status line.
* Each body part is either DICOM XML metadata or a bulk data item from a SOP Instance sent as part of the Store operation.

The first part of the multipart message must be XML metadata and contains the following HTTP headers:

* Content-Type: application/dicom+xml; transfer-syntax = {TransferSyntaxUID}

Subsequent items will contain the following HTTP headers (order is not guaranteed):

* Content-Type: application/dicom+xml; transfer-syntax={TransferSyntaxUID}

An uncompressed bulk data element encoded in Little Endian binary format with the following headers:

* Content-Type: application/octet-stream

Content-Location: {BulkDataURI}

A compressed pixel data object from a SOP Instance in the Study with the following headers:

* Content-Type: {MediaType}

Content-Location: {BulkDataURI}

Metadata and its associated bulk data shall always be sent in the same POST request.

**2). Validation of STOW request and DICOM file header**

* Firstly, the format of Study Instance ID in the STOW – RS request URL should be validated.
* Secondly, the Study Instance ID of the STOW- RS request URL should be checked for consistency with the Study Instance ID field of the DICOM file header.
* Thirdly, the header of the DICOM file, consisting of the 128 bytes of preamble, 4 bytes of prefix, and the data set (comprising of data elements) should be checked.
* This module is also coded in C#.

**3). Ensuring security**

* Mechanism for storing DICOM persistent objects via STOW-RS will be through HTTPS protocol, using DICOM UIDs for Study/Series/SOP Instance level.
* HTTP BASIC Authorization over SSL is supported.
* Deployment of trusted SSL Client and Server Certificates on the client and the sever machine (upon which STOW-RS is deployed). Trusted Client and Server certificates are used for integration and testing purposes only.
* A set of existing trusted Client, Server, Issuer CA, and Root CA certificates are used to set up HTTPS using the Microsoft Management Console.
* The code for HTTPS binding is written in C#.

**4). Storing the files**


* This module creates new resources for the given DICOM instances on the Server or appends them to an existing resource on the Server.
* One or more DICOM instances associated with one or more study instance unique identifiers (SUID) are stored in the appropriate file store location.
* The Storage Library is responsible for the physical storing of DICOM files, independent of the underlying storage architecture (NAS, SAN, or NFS).
* This module is coded in C++/CLI.


**5). Issuing a HTTP Response Message**

* The STOW-RS RESTful Service shall return an HTTP status line, including a status code and associated textual phrase for the entire set of stored SOP Instances, followed by a message body containing the Store Instances Response Module.
* If the status for all instances included in the POST request is Success, the RESTful Service shall return an "HTTP 200 - Success “response code.
* If the status for all instances included in the POST request is Failure, the RESTful Service shall return an appropriate failure status line with a response code.
* If there are instance specific errors, the response code shall be a 409 and the response payload shall contain the Store Instances Response Module, which contains additional information regarding instance errors.
* In all other conditions, the RESTful Service shall return an "HTTP 202 - Accepted" response code.
* The response payload may contain Store Instances Response Module, which specifies additional information regarding instance warnings or failures.
* This module is written in C#.

The standard HTTP response codes are listed in Table .1:

**Table 1:** HTTP/1.1 STANDARD RESPONSE CODE





**V. CONCLUSION**

The implementation details of STOW-RS were described in this document. Due to the proprietary nature of this project, the minor details of implementation cannot be revealed. Also, due to the adoption of the Scaled Agile Process Model, the implementation will continue to evolve in the next increment.